Nikon CoolPix P610

#### Effective Pixels

16.0 million

#### Sensor Size

1/2.3 in.

#### Monitor Size

3.0 in. diagonal

#### Monitor Type

TFT-LCD with Anti-reflection coating  
6-level brightness adjustment

#### Storage Media

SD memory card  
SDHC memory card  
SDXC memory card

#### Movie

Full HD: 1920x1080/ 60p  
Full HD: 1920x1080/ 50p  
Full HD: 1920x1080/ 30p  
Full HD: 1920x1080/ 25p  
HD: 1280x720/ 60p  
HD: 1280x720/ 50p  
HD: 1280x720/ 30p  
HD: 1280x720/ 25p  
HS 1920x1080/ 15p  
HS 1280x720/ 50p  
HS 1280x720/ 60p  
HS 1920x1080/ 12.5p  
HS 640x480/ 100p  
VGA 640x480/ 30p  
VGA 640x480/ 25p  
HS 640x480/ 120p

#### ISO Sensitivity

ISO 100-1600  
ISO 3200, 6400 (available when using P, S, A or M mode)  
ISO Hi 1 (equivalent to ISO 12,800) (available when using High ISO monochrome in special effects mode)

#### Top Continuous Shooting Speed at full resolution

Up to 7 shots at approx. 7frames per second

#### Battery / Batteries

Rechargeable Li-ion Battery EN-EL23

#### Approx. Dimensions (Width x Height x Depth)

5.0 in. (125.0 mm) x 3.4in. (85.0 mm) x 4.2 in.(106.5 mm)excluding projections