Nikon CoolPix P340

#### Effective Pixels

12.2 million

#### Sensor Size

1/1.7 in.

#### Monitor Size

3.0 in. diagonal

#### Monitor Type

Wide Viewing AngleTFT-LCD with Anti-reflection coating  
6-level brightness adjustment

#### Storage Media

SD memory card  
SDHC memory card  
SDXC memory card

#### Movie

Full HD: 1920x1080/ 30p  
Full HD: 1920x1080/ 25p  
Full HD: 1920x1080/ 60i  
Full HD: 1920x1080/ 50i  
HD: 1280x720/ 30p  
HD: 1280x720/ 25p  
HS 1920x1080/ 15p  
HS 1280x720/ 50p  
HS 1280x720/ 60p  
HS 1920x1080/ 12.5p  
HS 640x480/ 100p  
HS 320x240/ 240p  
HS 640x480/ 120p  
iFrame 720/ 30p  
iFrame 720/ 25p  
VGA 640x480/ 30p  
VGA 640x480/ 25p

#### ISO Sensitivity

ISO 80-3200  
ISO 6400, Hi 1 (equivalent to ISO 12,800) (available when using P, S, A, or M mode)  
Hi 2 (equivalent to ISO 25,600) (available when using High ISO monochrome in special effects mode)

#### Top Continuous Shooting Speed at full resolution

Up to 10 shots at approx.10 frames per second

#### Battery / Batteries

Rechargeable Li-ion Battery EN-EL12

#### Approx. Dimensions (Width x Height x Depth)

4.1 in. (103.0 mm) x 2.3in. (58.3 mm) x 1.3 in.(32.0 mm)excluding projections